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Burning Magnesium Oxide
Burning Magnesium Oxide Caustic Calcined Magnesite

It is made from magnesite ore as raw material, by calcining in rotary kiln, manufactured after fine grinding, stable quality performance, high purity, good activity. It is extensively applied to produce refractory materials, chemical engineering, building material and paper making industry, etc.
 
Burning Magnesium Oxide Description

Magnesium oxide is white or light yellow powder. It is tasteless, nontoxic amorphous.
It is slightly soluble in white and organic solvents, and soluble in acid or salt solution.
Burning Magnesium Oxide Packing
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1MT/net by PP bags , 1.25MT/net by PP bags or as per customer's request.
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Burning Magnesium Oxide Description Capacity
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18MT/20MT/25MT into one 20 FCL
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